evid

Base Table | request_card
Attribute Name | evid
ColumnName | evid
RoleName |
Definition | Event identifier. Each event is assigned a unique integer which identifies it in a database
Note | Range: evid > 0

auth

Base Table | request_card
Attribute Name | auth
ColumnName | auth
RoleName |
Definition | The auth field specifies the source of the information. This may be a network identifier (FDSN or otherwise), or any other string indicating the source of the information in the record
Note | Range: Any free-format string up to 15 characters

subsource

Base Table | request_card
Attribute Name | subsource
ColumnName | subsource
RoleName |
Definition | A second identifier to specify the system or process that derived the data. e.g., the origin's AUTH is CI, but the subsource (the solution) was computed by JIGGLE
Note | Range: Any free-format string up to 8 characters

net

Base Table | request_card
Attribute Name | net
ColumnName | net
RoleName |
Definition | Unique network identifier. This character string is the name of a seismic network
Note | Range: Any free-format string up to 8 characters. If available, use the two character FDSN code for the network

sta

Base Table | request_card
Attribute Name | sta
ColumnName | sta
RoleName |
Definition | Station code. This is the common code-name of a seismic observatory. Generally only three or four characters are used
Note | Range: Any free-format string up to 6 characters

seedchan

Base Table | request_card
Attribute Name | seedchan
ColumnName | seedchan
RoleName |
Definition | SEED channel name. The first character denotes the band code, the second for the instrument code and the third represents the component code
Note | Range: seedchan = {E | S | H | B | M | L | V | U | R} U {A | B | D | F | G | H | I | K | L | M | P | R | S | V | T | W} U {Z | N | E | A | B | C | T | R | 1 | 2 | 3 | U | V | W} Band code: Sample rate (Hz) Corner period (sec) E = extremely short period ³ 80 < 10 S = short period ³ 10 to < 80 < 10 H = high broad band ³ 80 ³ 10 B = broad band ³ 10 to < 80 ³ 10 M = mid period > 1 to < 10 L = long period ~ 1 V = very long period ~ 0.1 U = ultra long period ~ 0.01 R = extremely long period ~ 0.001 Instrument code: A = tiltmeter B = creepmeter D = pressure F = magnetometer G = gravimeter/accelerometer H = high gain seismometer I = humidity K = temperature L = low gain seismometer M = mass position seismometer P = geophone R = rainfall S = linear strainmeter V = volumetric strain T = tide meter W = wind Component code: N = north-south E = east-west T = transverse R = radial Z = vertical A, B, C = triaxial 1, 2, 3 = orthogonal components but non-traditional orientations U, V, W = optional components

staauth

Base Table | request_card
Attribute Name | staauth
ColumnName | staauth
RoleName |
Definition | Purpose unknown (always same as subsource)
Note | Range: Any free-format string up to 15 characters long

channel

Base Table | request_card
Attribute Name | channel
ColumnName | channel
RoleName |
Definition | Channel name
Note | Range: Any valid channel name, which may be network-specific. Networks using SEED channel names should use the same value for channel and seedchan

datetime_on

Base Table | request_card
Attribute Name | datetime_on
ColumnName | datetime_on
RoleName |
Definition | Start time of time window to save
Note | Range: Any valid float. datetime = 0.0 on January 01, 1970 at 00:00:00.0000 Units: Seconds

datetime_off

Base Table | request_card
Attribute Name | datetime_off
ColumnName | datetime_off
RoleName |
Definition | End time of time window to save
Note | Range: Any valid float. datetime = 0.0 on January 01, 1970 at 00:00:00.0000 Units: Seconds

request_type

Base Table | request_card
Attribute Name | request_type
ColumnName | request_type
RoleName |
Definition | Single character flag describing request type
Note | Range: request_type = {T | C} T = trigger, C = continuous

lddate

Base Table | request_card
Attribute Name | lddate
ColumnName | lddate
RoleName |
Definition | Load date. Date and time that the record was created or last modified, in Oracle date datatype
Note | Range: Any valid date between January 01, 4712 BC and January 01, 4712 AD Units: YYYY/MM/DD HH24:MI:SS

rcid

Base Table | request_card
Attribute Name | rcid
ColumnName | rcid
RoleName |
Definition | Unique request row number. Derived from REQSEQ.
Note | Range: rcid > 0

location

Base Table | request_card
Attribute Name | location
ColumnName | location
RoleName |
Definition | Describes the individual sites on an array station, operated by the same network operator
Note | Range: Any free-format string up to 2 characters long

retry

Base Table | request_card
Attribute Name | retry
ColumnName | retry
RoleName |
Definition | Count of attempts to retrieve this waveform
Note | Range: retry > 0

lastretry

Base Table | request_card
Attribute Name | lastretry
ColumnName | lastretry
RoleName |
Definition | Time of last attempt to retrieve this waveform
Note | Range: Any valid date between January 01, 4712 BC and January 01, 4712 AD Units: YYYY/MM/DD HH24:MI:SS

priority

Base Table | request_card
Attribute Name | priority
ColumnName | priority
RoleName |
Definition | Rows are processed in priority order, 1 is highest priority
Note | Range: priority > 0