evid

Base Entity | request_card
Attribute Name | evid
Logical Rolename |
ColumnName | EVID
RoleName |
Definition |
    Event identifier. Each event is assigned a unique integer which identifies it in a database
Note |
    Range: evid > 0

auth

Base Entity | request_card
Attribute Name | auth
Logical Rolename |
ColumnName | AUTH
RoleName |
Definition |
    The auth field specifies the source of the information. This may be a network identifier (FDSN or otherwise), or any other string indicating the source of the information in the record
Note |
    Range: Any free-format string up to 15 characters

subsource

Base Entity | request_card
Attribute Name | subsource
Logical Rolename |
ColumnName | SUBSOURCE
RoleName |
Definition |
    A second identifier to specify the system or process that derived the data. e.g., the origin's AUTH is CI, but the subsource (the solution) was computed by JIGGLE
Note |
    Range: Any free-format string up to 8 characters

net

Base Entity | request_card
Attribute Name | net
Logical Rolename |
ColumnName | NET
RoleName |
Definition |
    Unique network identifier. This character string is the name of a seismic network
Note |
    Range: Any free-format string up to 8 characters. If available, use the two character FDSN code for the network

sta

Base Entity | request_card
Attribute Name | sta
Logical Rolename |
ColumnName | STA
RoleName |
Definition |
    Station code. This is the common code-name of a seismic observatory. Generally only three or four characters are used
Note |
    Range: Any free-format string up to 6 characters

seedchan

Base Entity | request_card
Attribute Name | seedchan
Logical Rolename |
ColumnName | SEEDCHAN
RoleName |
Definition |
    SEED channel name. The first character denotes the band code, the second for the instrument code and the third represents the component code
Note |
    Range: seedchan = {E | S | H | B | M | L | V | U | R} U {A | B | D | F | G | H | I | K | L | M | P | R | S | V | T | W} U {Z | N | E | A | B | C | T | R | 1 | 2 | 3 | U | V | W} Band code: Sample rate (Hz) Corner period (sec) E = extremely short period ³ 80 < 10 S = short period ³ 10 to < 80 < 10 H = high broad band ³ 80 ³ 10 B = broad band ³ 10 to < 80 ³ 10 M = mid period > 1 to < 10 L = long period ~ 1 V = very long period ~ 0.1 U = ultra long period ~ 0.01 R = extremely long period ~ 0.001 Instrument code: A = tiltmeter B = creepmeter D = pressure F = magnetometer G = gravimeter/accelerometer H = high gain seismometer I = humidity K = temperature L = low gain seismometer M = mass position seismometer P = geophone R = rainfall S = linear strainmeter V = volumetric strain T = tide meter W = wind Component code: N = north-south E = east-west T = transverse R = radial Z = vertical A, B, C = triaxial 1, 2, 3 = orthogonal components but non-traditional orientations U, V, W = optional components

staauth

Base Entity | request_card
Attribute Name | staauth
Logical Rolename |
ColumnName | STAAUTH
RoleName |
Definition |
    Purpose unknown (always same as subsource)
Note |
    Range: Any free-format string up to 15 characters long

channel

Base Entity | request_card
Attribute Name | channel
Logical Rolename |
ColumnName | CHANNEL
RoleName |
Definition |
    Channel name
Note |
    Range: Any valid channel name, which may be network-specific. Networks using SEED channel names should use the same value for channel and seedchan

datetime_on

Base Entity | request_card
Attribute Name | datetime_on
Logical Rolename |
ColumnName | DATETIME_ON
RoleName |
Definition |
    Start time of time window to save
Note |
    Range: Any valid float. datetime = 0.0 on January 01, 1970 at 00:00:00.0000 Units: Seconds

datetime_off

Base Entity | request_card
Attribute Name | datetime_off
Logical Rolename |
ColumnName | DATETIME_OFF
RoleName |
Definition |
    End time of time window to save
Note |
    Range: Any valid float. datetime = 0.0 on January 01, 1970 at 00:00:00.0000 Units: Seconds

request_type

Base Entity | request_card
Attribute Name | request_type
Logical Rolename |
ColumnName | REQUEST_TYPE
RoleName |
Definition |
    Single character flag describing request type
Note |
    Range: request_type = {T | C} T = trigger, C = continuous

lddate

Base Entity | request_card
Attribute Name | lddate
Logical Rolename |
ColumnName | LDDATE
RoleName |
Definition |
    Load date. Date and time that the record was created or last modified, in Oracle date datatype
Note |
    Range: Any valid date between January 01, 4712 BC and January 01, 4712 AD Units: YYYY/MM/DD HH24:MI:SS

rcid

Base Entity | request_card
Attribute Name | rcid
Logical Rolename |
ColumnName | RCID
RoleName |
Definition |
    Unique request row number. Derived from REQSEQ.
Note |
    Range: rcid > 0

location

Base Entity | request_card
Attribute Name | location
Logical Rolename |
ColumnName | LOCATION
RoleName |
Definition |
    Describes the individual sites on an array station, operated by the same network operator
Note |
    Range: Any free-format string up to 2 characters long

retry

Base Entity | request_card
Attribute Name | retry
Logical Rolename |
ColumnName | RETRY
RoleName |
Definition |
    Count of attempts to retrieve this waveform
Note |
    Range: retry > 0

lastretry

Base Entity | request_card
Attribute Name | lastretry
Logical Rolename |
ColumnName | LASTRETRY
RoleName |
Definition |
    Time of last attempt to retrieve this waveform
Note |
    Range: Any valid date between January 01, 4712 BC and January 01, 4712 AD Units: YYYY/MM/DD HH24:MI:SS

priority

Base Entity | request_card
Attribute Name | priority
Logical Rolename |
ColumnName | PRIORITY
RoleName |
Definition |
    Rows are processed in priority order, 1 is highest priority
Note |
    Range: priority > 0