sta

Base Table | Station_Sensor
Attribute Name | sta
ColumnName | sta
Logical Rolename |
RoleName |
Definition | Station code. This is the common code-name of a seismic observatory. Generally only three or four characters are used
Note |

net

Base Table | Station_Sensor
Attribute Name | net
ColumnName | net
Logical Rolename |
RoleName |
Definition | Unique network identifier. This character string is the name of a seismic network
Note |

sensor_nb

Base Table | Station_Sensor
Attribute Name | sensor_nb
ColumnName | sensor_nb
Logical Rolename |
RoleName |
Definition | This attribute represents the sensor number
Note |

ondate

Base Table | Station_Sensor
Attribute Name | ondate
ColumnName | ondate
Logical Rolename |
RoleName |
Definition | This attribute denotes the start date
Note |

sensor_id

Base Table | Station_Sensor
Attribute Name | sensor_id
ColumnName | sensor_id
Logical Rolename |
RoleName |
Definition | Sensor identifier. Each sensor is assigned a unique integer which identifies it in a database
Note |

lat

Base Table | Station_Sensor
Attribute Name | lat
ColumnName | lat
Logical Rolename |
RoleName |
Definition | Latitude. This attribute is the geographic latitude. Locations north of the equator have positive latitudes
Note |

lon

Base Table | Station_Sensor
Attribute Name | lon
ColumnName | lon
Logical Rolename |
RoleName |
Definition | Longitude. This attribute is the geographic longitude. Longitudes are measured positive east of the Greenwich meridian
Note |

elev

Base Table | Station_Sensor
Attribute Name | elev
ColumnName | elev
Logical Rolename |
RoleName |
Definition | Elevation. This attribute is the elevation of a seismic station relative to mean sea level
Note |

edepth

Base Table | Station_Sensor
Attribute Name | edepth
ColumnName | edepth
Logical Rolename |
RoleName |
Definition | Emplacement depth. This attribute gives the depth at which the instrument is positioned, relative to the value of elev
Note |

nb_component

Base Table | Station_Sensor
Attribute Name | nb_component
ColumnName | nb_component
Logical Rolename |
RoleName |
Definition | This attribute denotes the number of components of a sensor
Note |

datumhor

Base Table | Station_Sensor
Attribute Name | datumhor
ColumnName | datumhor
Logical Rolename |
RoleName |
Definition | Datum type for horizontal (latitude and longitude) coordinates
Note |

datumver

Base Table | Station_Sensor
Attribute Name | datumver
ColumnName | datumver
Logical Rolename |
RoleName |
Definition | Datum type for depth or elevation
Note |

offdate

Base Table | Station_Sensor
Attribute Name | offdate
ColumnName | offdate
Logical Rolename |
RoleName |
Definition | This attribute denotes the end date
Note |

lddate

Base Table | Station_Sensor
Attribute Name | lddate
ColumnName | lddate
Logical Rolename |
RoleName |
Definition | Load date. Date and time that the record was created or last modified, in Oracle date datatype
Note |