arid

Base Table | arrival
Attribute Name | arid
ColumnName | arid
Logical Rolename |
RoleName |
Definition | Arrival identifier. Each arrival is assigned a unique positive integer identifying it. This number is used in the AssocArO relation along with the origin identifier to link Arrival and Origin
Note |
    Range:             arid > 0

commid

Base Table | arrival
Attribute Name | commid
ColumnName | commid
Logical Rolename |
RoleName |
Definition | Comment identification. This is a key used to point to free-form comments entered in the Remark relation. These comments store additional information about a tuple in another relation. Within the Remark relation, there may be many tuples with the same commid and different lineno, but the same commid will appear in only one other tuple among the rest of the relations in the database
Note |
    Range:             commid > 0

datetime

Base Table | arrival
Attribute Name | datetime
ColumnName | datetime
Logical Rolename |
RoleName |
Definition | The date of associated with information in the record, in true epoch format
Note |
    Range:		Any valid float. datetime = 0.0 on January 01, 1970 at 00:00:00.0000

    Units:		Seconds

sta

Base Table | arrival
Attribute Name | sta
ColumnName | sta
Logical Rolename |
RoleName |
Definition | Station code. This is the common code-name of a seismic observatory. Generally only three or four characters are used
Note |
    Range:             Any free-format string up to 6 characters

net

Base Table | arrival
Attribute Name | net
ColumnName | net
Logical Rolename |
RoleName |
Definition | Unique network identifier. This character string is the name of a seismic network
Note |
    Range:             Any free-format string up to 8 characters. If available, use the two character FDSN code for the network

auth

Base Table | arrival
Attribute Name | auth
ColumnName | auth
Logical Rolename |
RoleName |
Definition | The auth field specifies the source of the information. This may be a network identifier (FDSN or otherwise), or any other string indicating the source of the information in the record
Note |
    Range:            Any free-format string up to 15 characters

subsource

Base Table | arrival
Attribute Name | subsource
ColumnName | subsource
Logical Rolename |
RoleName |
Definition | A second identifier to specify the system or process that derived the data. e.g., the origin's AUTH is CI, but the subsource (the solution) was computed by JIGGLE. Contains hypoinverse station card column 109 for historic catalogs
Note |
    Range:             Any free-format string up to 8 characters

channel

Base Table | arrival
Attribute Name | channel
ColumnName | channel
Logical Rolename |
RoleName |
Definition | Channel name
Note |
    Range:             	Any valid channel name, which may be network-specific. Networks using SEED channel names should use the same value for channel and seedchan

channelsrc

Base Table | arrival
Attribute Name | channelsrc
ColumnName | channelsrc
Logical Rolename |
RoleName |
Definition | Domain for channel. This specifies what naming convention is used for the channel name (i.e. SEED, USGS, etc.)
Note |
    Range:             Any free-format string up to 8 characters long

seedchan

Base Table | arrival
Attribute Name | seedchan
ColumnName | seedchan
Logical Rolename |
RoleName |
Definition | SEED channel name. The first character denotes the band code, the second for the instrument code and the third represents the component code
Note |
    Range:		seedchan = {E | S | H | B | M | L | V | U | R} U
    		                   {A | B | D | F | G | H | I | K | L | M | P | R | S | V | T | W} U
    		                   {Z | N | E | A | B | C | T | R | 1 | 2 | 3 | U | V | W}
    		Band code:
    						Sample rate (Hz)	Corner period (sec)
    		E = extremely short period		³ 80			< 10
    		S = short period			³ 10 to < 80		< 10
    		H = high broad band		³ 80			³ 10
    		B = broad band			³ 10 to < 80		³ 10
    		M = mid period			> 1 to < 10
    		L = long period			~ 1
    		V = very long period			~ 0.1
    		U = ultra long period			~ 0.01
    		R = extremely long period		~ 0.001

    		Instrument code:
    		A = tiltmeter			B = creepmeter
    		D = pressure			F = magnetometer
    		G = gravimeter/accelerometer		H = high gain seismometer
    		I = humidity			K = temperature
    		L = low gain seismometer		M = mass position seismometer
    		P = geophone			R = rainfall
    		S = linear strainmeter		V = volumetric strain
    		T = tide meter			W = wind

    		Component code:
    		N = north-south		E = east-west
    		T = transverse		R = radial
    		Z = vertical
    		A, B, C = triaxial
    		1, 2, 3 = orthogonal components but non-traditional orientations
    		U, V, W = optional components

location

Base Table | arrival
Attribute Name | location
ColumnName | location
Logical Rolename |
RoleName |
Definition | Describes the individual sites on an array station, operated by the same network operator
Note |
    Range:             Any free-format string up to 2 characters long

iphase

Base Table | arrival
Attribute Name | iphase
ColumnName | iphase
Logical Rolename |
RoleName |
Definition | Reported phase. This eight-character field holds the name initially given to a seismic phase. Standard seismological labels for the types of signals (or phases) are used (e.g., P, PKP, PcP, pP). Both upper and lower case letters are available and should be used when appropriate, for example, pP or PcP
Note |
    Range:            Any free-format string up to 8 characters

qual

Base Table | arrival
Attribute Name | qual
ColumnName | qual
Logical Rolename |
RoleName |
Definition | Onset quality. This single-character flag is used to denote the sharpness of the onset of a seismic phase. This attribute does not denote the timing accuracy
Note |
    Range:		qual = {i | e | w}
    		i = impulsive
    		e = emergent
    		w = weak

clockqual

Base Table | arrival
Attribute Name | clockqual
ColumnName | clockqual
Logical Rolename |
RoleName |
Definition | This field describes whether the clock quality associated with a particular arrival is known, and if so, is good or bad
Note |
    Range:		clockqual = {U | G | B}
    		U = unknown
    		G = good
    		B = bad

clockcorr

Base Table | arrival
Attribute Name | clockcorr
ColumnName | clockcorr
Logical Rolename |
RoleName |
Definition | This field indicates the amount of time to add to the arrival time if clock correction is known
Note |
    Units:		Microseconds

ccset

Base Table | arrival
Attribute Name | ccset
ColumnName | ccset
Logical Rolename |
RoleName |
Definition | This field describes whether the clock correction has been added or applied to the arrivals in computing a hypocenter solution
Note |
    Range:		ccset in {0 | 1}
    		0 = no
    		1 = yes

fm

Base Table | arrival
Attribute Name | fm
ColumnName | fm
Logical Rolename |
RoleName |
Definition | First motion. This is a two-character indication of first motion. The first character describes first motion seen on short-period channels and the second holds for long-period instruments. Compression (dilation) on a short-period sensor is denoted by c(d) and compression (dilation) on a long-period sensor is denoted by u(r). Empty character positions will be indicated by dots (e.g., ".r"). Lower quality first motions can be described by +(-)
Note |
    Range:             All two-letter permutations of (c | d | + | - | .} U {u | r | .}

ema

Base Table | arrival
Attribute Name | ema
ColumnName | ema
Logical Rolename |
RoleName |
Definition | Emergence angle. This attribute is the emergence angle of an arrival, as observed at a three-component station or array. The value increases from the vertical direction towards the horizontal
Note |
    Range:		0.0 <= ema <= 90.0

    Units:		Degrees

azimuth

Base Table | arrival
Attribute Name | azimuth
ColumnName | azimuth
Logical Rolename |
RoleName |
Definition | Station to event azimuth measured clockwise from true north. Identified from waveform analysis
Note |
    Range:		0.0 <= azimuth <= 360.0

    Units:		Degrees

slow

Base Table | arrival
Attribute Name | slow
ColumnName | slow
Logical Rolename |
RoleName |
Definition | Observed slowness. This is the observed slowness of a wave as it sweeps across an array
Note |
    Range:		slow >= 0.0

    Units:		Seconds/kilometer

deltim

Base Table | arrival
Attribute Name | deltim
ColumnName | deltim
Logical Rolename |
RoleName |
Definition | Arrival time uncertainty. This attribute gives the standard deviation of a detection time
Note |
    Range:		deltim >= 0.0

    Units:		Seconds

delinc

Base Table | arrival
Attribute Name | delinc
ColumnName | delinc
Logical Rolename |
RoleName |
Definition | Uncertainty in the angle. This attribute gives the standard deviation of the angle of emergence
Note |
    Range:		delinc >= 0.0

    Units:		Degrees

delaz

Base Table | arrival
Attribute Name | delaz
ColumnName | delaz
Logical Rolename |
RoleName |
Definition | Uncertainty in the azimuth. This attribute gives the standard deviation of the azimuth of a signal
Note |
    Range:		delaz > 0.0

    Units:		Degrees

delslo

Base Table | arrival
Attribute Name | delslo
ColumnName | delslo
Logical Rolename |
RoleName |
Definition | Uncertainty in slowness. This attribute gives the standard deviation of the slowness of a signal
Note |
    Range:		delslo > 0.0

    Units:		Seconds/Kilometers

quality

Base Table | arrival
Attribute Name | quality
ColumnName | quality
Logical Rolename |
RoleName |
Definition | This attribute denotes the quality of an origin, an arrival, or a mechanism. 1.0 = good, 0.0 = bad. Hypoinverse station archive card columns 17 & 50: 0, 5 --> 1.00 1, 6 --> 0.75 2, 7 --> 0.50 3, 8 --> 0.25 4, 9 --> 0.00
Note |
    Range:             0.0 <= quality <= 1.0

snr

Base Table | arrival
Attribute Name | snr
ColumnName | snr
Logical Rolename |
RoleName |
Definition | Signal-to-noise ratio. This is an estimate of the signal relative to that of the noise immediately preceding it
Note |
    Range:             snr > 0.0

rflag

Base Table | arrival
Attribute Name | rflag
ColumnName | rflag
Logical Rolename |
RoleName |
Definition | This flag describes whether an observation was generated automatically, by a human, or has been finalized
Note |
    Range:		rflag = {A | H | F}
    		A = automatic
    		H = reviewed by human
    		F = finalized

lddate

Base Table | arrival
Attribute Name | lddate
ColumnName | lddate
Logical Rolename |
RoleName |
Definition | Load date. Date and time that the record was created, in Oracle date datatype
Note |
    Range:		Any valid date between January 01, 4712 BC and January 01, 4712 AD

    Units:		 YYYY/MM/DD HH24:MI:SS