orid

Base Object | assocaro
Attribute Name | orid
ColumnName | orid
Logical Rolename |
RoleName |
Definition | Origin identification. Each origin is assigned a unique positive integer which identifies it in the database. The orid is used to identify one of the many hypotheses of the actual location of the event
Note |
    Range:             orid > 0

arid

Base Object | assocaro
Attribute Name | arid
ColumnName | arid
Logical Rolename |
RoleName |
Definition | Arrival identifier. Each arrival is assigned a unique positive integer identifying it. This number is used in the AssocArO relation along with the origin identifier to link Arrival and Origin
Note |
    Range:             arid > 0

commid

Base Object | assocaro
Attribute Name | commid
ColumnName | commid
Logical Rolename |
RoleName |
Definition | Comment identification. This is a key used to point to free-form comments entered in the Remark relation. These comments store additional information about a tuple in another relation. Within the Remark relation, there may be many tuples with the same commid and different lineno, but the same commid will appear in only one other tuple among the rest of the relations in the database
Note |
    Range:             commid > 0

auth

Base Object | assocaro
Attribute Name | auth
ColumnName | auth
Logical Rolename |
RoleName |
Definition | The auth field specifies the source of the information. This may be a network identifier (FDSN or otherwise), or any other string indicating the source of the information in the record
Note |
    Range:            Any free-format string up to 15 characters

subsource

Base Object | assocaro
Attribute Name | subsource
ColumnName | subsource
Logical Rolename |
RoleName |
Definition | A second identifier to specify the system or process that derived the data. e.g., the origin's AUTH is CI, but the subsource (the solution) was computed by JIGGLE
Note |
    Range:             Any free-format string up to 8 characters

iphase

Base Object | assocaro
Attribute Name | iphase
ColumnName | iphase
Logical Rolename |
RoleName |
Definition | Reported phase. This eight-character field holds the name initially given to a seismic phase. Standard seismological labels for the types of signals (or phases) are used (e.g., P, PKP, PcP, pP). Both upper and lower case letters are available and should be used when appropriate, for example, pP or PcP
Note |
    Range:            Any free-format string up to 8 characters

importance

Base Object | assocaro
Attribute Name | importance
ColumnName | importance
Logical Rolename |
RoleName |
Definition | This attribute denotes the importance of a phase/amplitude reading towards an origin/magnitude. 0.0 means no importance, 1.0 implies extremely important
Note |
    Range:             0.0 < importance <= 1.0

delta

Base Object | assocaro
Attribute Name | delta
ColumnName | delta
Logical Rolename |
RoleName |
Definition | Source-receiver distance. This attribute is the arc length, over the earth’s surface, of the path the seismic phase follows from source to receiver. The location of the origin is specified in the origin record referenced by the attribute orid. The attribute arid points to the record in the Arrival relation that identifies the receiver.
Note |
    Range:		delta >= 0.0

    Units:		Kilometers

seaz

Base Object | assocaro
Attribute Name | seaz
ColumnName | seaz
Logical Rolename |
RoleName |
Definition | Event to station azimuth. This attribute is calculated from the event and station locations. It is measured clockwise from North
Note |
    Range:		0.0 <= seaz <= 360.0

    Units:		Degrees

in_wgt

Base Object | assocaro
Attribute Name | in_wgt
ColumnName | in_wgt
Logical Rolename |
RoleName |
Definition | Input weight. Hypoinverse station archive card columns 17 & 50: 0, 1, 2, 3 --> 1.00 4, 5, 6, 7, 8, 9 --> 0.00
Note |
    Range:		0.0 < in_wgt <= 1.0
    		0.0 = no weight (not used)

wgt

Base Object | assocaro
Attribute Name | wgt
ColumnName | wgt
Logical Rolename |
RoleName |
Definition | Location weight. This attribute gives the final weight assigned to the allied arrival by the location program. It is used primarily for location programs that adaptively weight data by their residuals. Raw values from hypoinverse columns 39 & 64
Note |

timeres

Base Object | assocaro
Attribute Name | timeres
ColumnName | timeres
Logical Rolename |
RoleName |
Definition | Time residual. This attribute is a travel time residual, measured in seconds. The residual is found by taking the observed arrival time (saved in the Arrival relation) of a seismic phase and substracting the expected arrival time. The expected arrival time is calculated by a formula based on earth velocity model, an event location and origin time, the distance to the station, and the particular seismic phase
Note |
    Range:		timeres >= 0.0

    Units:		Seconds

ema

Base Object | assocaro
Attribute Name | ema
ColumnName | ema
Logical Rolename |
RoleName |
Definition | The takeoff angle at the source, measured in degrees, with vertical down. ema=0 leaves the source straight down, while ema=180 leaves the source straight up; calculated in hypoinverse using the velocity model
Note |
    Range:0 <= ema <= 180

    Units:Degrees

slow

Base Object | assocaro
Attribute Name | slow
ColumnName | slow
Logical Rolename |
RoleName |
Definition | Slowness residual. This attribute gives the difference between an observed slowness (saved in the Arrival relation) and a theorical prediction. The prediction is calculated for the related phase and event origin described in the record
Note |
    Range:		slow >= 0.0

    Units:		Seconds/kilometer

vmodelid

Base Object | assocaro
Attribute Name | vmodelid
ColumnName | vmodelid
Logical Rolename |
RoleName |
Definition | Velocity model identification
Note |
    Range:             vmodelid > 0

scorr

Base Object | assocaro
Attribute Name | scorr
ColumnName | scorr
Logical Rolename |
RoleName |
Definition | Station correction
Note |
    Range:		Any valid float

    Units:		Seconds

sdelay

Base Object | assocaro
Attribute Name | sdelay
ColumnName | sdelay
Logical Rolename |
RoleName |
Definition | Station delay
Note |
    Range:		Any valid float

    Units:		Seconds

rflag

Base Object | assocaro
Attribute Name | rflag
ColumnName | rflag
Logical Rolename |
RoleName |
Definition | This flag describes whether an observation was generated automatically, by a human, or has been finalized
Note |
    Range:		rflag = {A | H | F}
    		A = automatic
    		H = reviewed by human
    		F = finalized

ccset

Base Object | assocaro
Attribute Name | ccset
ColumnName | ccset
Logical Rolename |
RoleName |
Definition | This field describes whether the clock correction has been added or applied to the arrivals in computing a hypocenter solution
Note |
    Range:		ccset in {0 | 1}
    		0 = no
    		1 = yes

lddate

Base Object | assocaro
Attribute Name | lddate
ColumnName | lddate
Logical Rolename |
RoleName |
Definition | Load date. Date and time that the record was created, in Oracle date datatype
Note |
    Range:		Any valid date between January 01, 4712 BC and January 01, 4712 AD

    Units:		 YYYY/MM/DD HH24:MI:SS