net

Base Entity | stacorrections
Attribute Name | net
Logical Rolename | net
ColumnName | net
RoleName | net
Definition | Unique network identifier. This character string is the name of a seismic network
Note | Range: Any free-format string up to 8 characters. If available, use the two character FDSN code for the network

sta

Base Entity | stacorrections
Attribute Name | sta
Logical Rolename | sta
ColumnName | sta
RoleName | sta
Definition | Station code. This is the common code-name of a seismic observatory. Generally only three or four characters are used
Note | Range: Any free-format string up to 6 characters

seedchan

Base Entity | stacorrections
Attribute Name | seedchan
Logical Rolename | seedchan
ColumnName | seedchan
RoleName | seedchan
Definition | SEED channel name. The first character denotes the band code, the second for the instrument code and the third represents the component code
Note | Range: seedchan = {E | S | H | B | M | L | V | U | R} U {A | B | D | F | G | H | I | K | L | M | P | R | S | V | T | W} U {Z | N | E | A | B | C | T | R | 1 | 2 | 3 | U | V | W} Band code: Sample rate (Hz) Corner period (sec) E = extremely short period ³ 80 < 10 S = short period ³ 10 to < 80 < 10 H = high broad band ³ 80 ³ 10 B = broad band ³ 10 to < 80 ³ 10 M = mid period > 1 to < 10 L = long period ~ 1 V = very long period ~ 0.1 U = ultra long period ~ 0.01 R = extremely long period ~ 0.001 Instrument code: A = tiltmeter B = creepmeter D = pressure F = magnetometer G = gravimeter/accelerometer H = high gain seismometer I = humidity K = temperature L = low gain seismometer M = mass position seismometer P = geophone R = rainfall S = linear strainmeter V = volumetric strain T = tide meter W = wind Component code: N = north-south E = east-west T = transverse R = radial Z = vertical A, B, C = triaxial 1, 2, 3 = orthogonal components but non-traditional orientations U, V, W = optional components

channel

Base Entity | stacorrections
Attribute Name | channel
Logical Rolename | channel
ColumnName | channel
RoleName | channel
Definition | Channel name
Note | Range: Any valid channel name, which may be network-specific. Networks using SEED channel names should use the same value for channel and seedchan

channelsrc

Base Entity | stacorrections
Attribute Name | channelsrc
Logical Rolename | channelsrc
ColumnName | channelsrc
RoleName | channelsrc
Definition | Domain for channel. This specifies what naming convention is used for the channel name (i.e. SEED, USGS, etc.)
Note | Range: Any free-format string up to 8 characters long

location

Base Entity | stacorrections
Attribute Name | location
Logical Rolename | location
ColumnName | location
RoleName | location
Definition | Describes the individual sites on an array station, operated by the same network operator
Note | Range: Any free-format string up to 2 characters long

auth

Base Entity | stacorrections
Attribute Name | auth
Logical Rolename | auth
ColumnName | auth
RoleName | auth
Definition | The auth field specifies the source of the information. This may be a network identifier (FDSN or otherwise), or any other string indicating the source of the information in the record
Note | Range: Any free-format string up to 15 characters

corr

Base Entity | stacorrections
Attribute Name | corr
Logical Rolename | corr
ColumnName | corr
RoleName | corr
Definition | This attribute denotes the correction for the magnitude specified in corr_type
Note |

corr_flag

Base Entity | stacorrections
Attribute Name | corr_flag
Logical Rolename | corr_flag
ColumnName | corr_flag
RoleName | corr_flag
Definition | This attribute denotes if the magnitude correction is the default value, a value that is still being updated, or a frozen value, which is no longer updated
Note |

corr_type

Base Entity | stacorrections
Attribute Name | corr_type
Logical Rolename | corr_type
ColumnName | corr_type
RoleName | corr_type
Definition | This attribute denotes the magnitude type for which the correction is valid
Note |

ondate

Base Entity | stacorrections
Attribute Name | ondate
Logical Rolename | ondate
ColumnName | ondate
RoleName | ondate
Definition | This attribute denotes the start date
Note | Range: Any valid date between January 01, 4712 BC and January 01, 4712 AD Units: YYYY/MM/DD HH24:MI:SS

offdate

Base Entity | stacorrections
Attribute Name | offdate
Logical Rolename | offdate
ColumnName | offdate
RoleName | offdate
Definition | This attribute denotes the end date
Note | Range: Any valid date between January 01, 4712 BC and January 01, 4712 AD Units: YYYY/MM/DD HH24:MI:SS

lddate

Base Entity | stacorrections
Attribute Name | lddate
Logical Rolename | lddate
ColumnName | lddate
RoleName | lddate
Definition | Load date. Date and time that the record was created or last modified, in Oracle date datatype
Note | Range: Any valid date between January 01, 4712 BC and January 01, 4712 AD Units: YYYY/MM/DD HH24:MI:SS