net

Base Table | Coefficients
Attribute Name | net
ColumnName | net
Logical Rolename |
RoleName |
Definition | Unique network identifier. This character string is the name of a seismic network
Note |

sta

Base Table | Coefficients
Attribute Name | sta
ColumnName | sta
Logical Rolename |
RoleName |
Definition | Station code. This is the common code-name of a seismic observatory. Generally only three or four characters are used
Note |

seedchan

Base Table | Coefficients
Attribute Name | seedchan
ColumnName | seedchan
Logical Rolename |
RoleName |
Definition | SEED channel name. The first character denotes the band code, the second for the instrument code and the third represents the component code
Note |

location

Base Table | Coefficients
Attribute Name | location
ColumnName | location
Logical Rolename |
RoleName |
Definition | Describes the individual sites on an array station, operated by the same network operator
Note |

ondate

Base Table | Coefficients
Attribute Name | ondate
ColumnName | ondate
Logical Rolename |
RoleName |
Definition | This attribute denotes the start date
Note |

stage_seq

Base Table | Coefficients
Attribute Name | stage_seq
ColumnName | stage_seq
Logical Rolename |
RoleName |
Definition | This attribute denotes the stage number
Note |

channel

Base Table | Coefficients
Attribute Name | channel
ColumnName | channel
Logical Rolename |
RoleName |
Definition | Channel name
Note |

channelsrc

Base Table | Coefficients
Attribute Name | channelsrc
ColumnName | channelsrc
Logical Rolename |
RoleName |
Definition | Domain for channel. This specifies what naming convention is used for the channel name (i.e. SEED, USGS, etc.)
Note |

offdate

Base Table | Coefficients
Attribute Name | offdate
ColumnName | offdate
Logical Rolename |
RoleName |
Definition | This attribute denotes the end date
Note |

dc_key

Base Table | Coefficients
Attribute Name | key
ColumnName | dc_key
Logical Rolename |
RoleName | dc_key
Definition | Response (Coefficients) key
Note |

unit_in

Base Table | Coefficients
Attribute Name | id
ColumnName | unit_in
Logical Rolename |
RoleName | unit_in
Definition | A unit lookup key that refers to the Units Abbreviation Dictionary for the units of the incoming to this stage of the filter. This signal will usually be ground motion, volts, or counts, depending on where it is in the filter system
Note |

unit_out

Base Table | Coefficients
Attribute Name | id
ColumnName | unit_out
Logical Rolename |
RoleName | unit_out
Definition | A unit lookup key that refers to the Units Abbreviation Dictionary for the stage’s output signal. Analog filters usually emit volts, and digital filters usually emit counts
Note |

tf_type

Base Table | Coefficients
Attribute Name | tf_type
ColumnName | tf_type
Logical Rolename |
RoleName |
Definition | A single character describing the type of stage
Note |

lddate

Base Table | Coefficients
Attribute Name | lddate
ColumnName | lddate
Logical Rolename |
RoleName |
Definition | Load date. Date and time that the record was created or last modified, in Oracle date datatype
Note |