net

Base Table | Station_Comment
Attribute Name | net
ColumnName | net
Logical Rolename |
RoleName |
Definition | Unique network identifier. This character string is the name of a seismic network
Note |

sta

Base Table | Station_Comment
Attribute Name | sta
ColumnName | sta
Logical Rolename |
RoleName |
Definition | Station code. This is the common code-name of a seismic observatory. Generally only three or four characters are used
Note |

ondate

Base Table | Station_Comment
Attribute Name | ondate
ColumnName | ondate
Logical Rolename |
RoleName |
Definition | This attribute denotes the start date
Note |

comment_id

Base Table | Station_Comment
Attribute Name | id
ColumnName | comment_id
Logical Rolename |
RoleName | comment_id
Definition | The comment code key of the associated Comment Description Dictionary
Note |

offdate

Base Table | Station_Comment
Attribute Name | offdate
ColumnName | offdate
Logical Rolename |
RoleName |
Definition | This attribute denotes the end date
Note |

comment_level

Base Table | Station_Comment
Attribute Name | comment_level
ColumnName | comment_level
Logical Rolename |
RoleName |
Definition | The numeric value (if any) associated with the Units of comment level in the same Comment Description Dictionary. Together, this numeric value, its units, and the Description of comment of the associated Comment Description, all describe a comment for the station/channel
Note |

lddate

Base Table | Station_Comment
Attribute Name | lddate
ColumnName | lddate
Logical Rolename |
RoleName |
Definition | Load date. Date and time that the record was created or last modified, in Oracle date datatype
Note |