etype

Base Table | assoctypecat
Attribute Name | etype
ColumnName | etype
Logical Rolename |
RoleName |
Definition | This attribute is used to identify the type of seismic event
Note |
    Range:		etype = {le | re | ts | se | lp | to | tr | vt | nt | qb | ce | ex | sh | sn | th | ve | co | df | av | ls | rb | rs | bc | pc | mi | st | uk | ot | lf | su | px}
    		le = local earthquake
    		re = regional earthquake
    		ts = teleseismic eartquake
    		se = slow earthquake
    		lp = long period volcanic earthquake
    		to = tornillo wavelet
    		tr = non-volcanic tremor
    		vt = volcanic tremor
    		nt = nuclear test
    		qb = quarry blast
    		ce = calibration
    		ex = generic chemical blast
    		sh = refraction/reflection survey shot
    		sn = sonic shockwave
    		th = thunder
    		ve = volcanic eruption
    		co = mine/tunnel collapse
    		df = debris flow/avalanche
    		av = snow/ice avalanche
    		ls =  landslide
    		rb = rockburst
    		rs = rockslide
    		bc = building collapse/demolition
    		pc = plane crash
    		mi = meteor/comet impact
    		st = subnet trigger
    		uk = unknown type
    		ot = other miscellaneous
    		lf = low frequency
    		su = surface event
    		px = probable blast

catid

Base Table | assoctypecat
Attribute Name | catid
ColumnName | catid
Logical Rolename |
RoleName |
Definition | Category identifier
Note |
    Range:		catid > 0