origin

Logical Entity Name | origin
Default Table Name | origin
Definition | Data on event location

origin Columns

ColumnName | Domain | Datatype | NULL | Definition
orid |  | NUMBER(15, 0) | NO | Origin identification. Each origin is assigned a unique positive integer which identifies it in the database. The orid is used to identify one of the many hypotheses of the actual location of the event
evid |  | NUMBER(15, 0) | NO | Event identifier. Each event is assigned a unique integer which identifies it in a database. It is possible for several records in the Origin relation to have the same evid. This indicates there are several opinions about the location of the event. The evid does not have to be identical to the local network’s event identifier, which is stored in the Origin table. This allows merging data for a single event from multiple sources without insisting that database evid is identical to the source’s local event identifier
prefmag |  | NUMBER(15, 0) | YES | Preferred magnitude. This attribute holds the magnitude identifier, magid, that points to the preferred magnitude for a seismic event or an origin
prefmec |  | NUMBER(15, 0) | YES | Preferred mechanism. This attribute holds the mechanism identifier, mecid, that points to the preferred mechanism for a seismic event or an origin
commid |  | NUMBER(15, 0) | YES | Comment identification. This is a key used to point to free-form comments entered in the Remark relation. These comments store additional information about a tuple in another relation. Within the Remark relation, there may be many tuples with the same commid and different lineno, but the same commid will appear in only one other tuple among the rest of the relations in the database
bogusflag |  | NUMBER(1, 0) | NO | This field describes whether an origin is bogus or not
datetime |  | NUMBER(25, 10) | NO | The date of associated with information in the record, in true epoch format
lat |  | NUMBER(9, 7) | NO | Latitude. This attribute is the geographic latitude. Locations north of the equator have positive latitudes
lon |  | NUMBER(10, 7) | NO | Longitude. This attribute is the geographic longitude. Longitudes are measured positive east of the Greenwich meridian
depth |  | NUMBER(7, 3) | YES | Distance in KM of the earthquake source below the geoid. Hypoinverse model types E, L or V are always geoid depths
mdepth |  | NUMBER(7, 3) | YES | Distance in KM of the earthquake source below the model surface. For model depths, all the recording stations are located at the top of the model and their elevations are not used. Model types T or H if uncorrected by depth datum are always model depths
type |  | VARCHAR2(2) | YES | Type of location
algorithm |  | VARCHAR2(15) | YES | Algorithm used. This is a brief textual description of the algorithm used to compute a seismic origin
algo_assoc |  | VARCHAR2(80) | YES | Association algorithm used. This is a textual description of the algorithm used for associating the data
auth |  | VARCHAR2(15) | NO | The auth field specifies the source of the information. This may be a network identifier (FDSN or otherwise), or any other string indicating the source of the information in the record
subsource |  | VARCHAR2(8) | YES | A second identifier to specify the system or process that derived the data. e.g., the origin's AUTH is CI, but the subsource (the solution) was computed by JIGGLE
datumhor |  | VARCHAR2(8) | YES | Datum type for horizontal (latitude and longitude) coordinates
datumver |  | VARCHAR2(8) | YES | Datum type for depth or elevation
gap |  | NUMBER(4, 1) | YES | Gap in azimuthal coverage
distance |  | NUMBER(7, 3) | YES | Distance from the origin to the nearest station
wrms |  | NUMBER(5, 3) | YES | This attribute denotes the weighted RMS
stime |  | NUMBER(6, 3) | YES | Origin time error. This attribute denotes the standard deviation of the origin time
erhor |  | NUMBER(7, 3) | YES | Horizontal error. This attribute denotes the location uncertainty that accompanies the location
sdep |  | NUMBER(7, 3) | YES | Depth error. This is the standard deviation of the depth estimate
erlat |  | NUMBER(7, 3) | YES | Error in latitude. This is the standard deviation of the latitude estimate
erlon |  | NUMBER(7, 3) | YES | Error in longitude. This is the standard deviation of the longitude estimate
totalarr |  | NUMBER(5, 0) | YES | Total number of phases in the database for the specified orid. This field signifies the number of P and S arrivals with non-zero input weights
totalamp |  | NUMBER(6, 0) | YES | Total number of amplitudes in the database for the specified orid. Not all amplitudes have to associated with all magnitudes or origins
ndef |  | NUMBER(5, 0) | YES | This attribute denotes the number of phases with non-zero output weights used in hypocenter calculation
nbs |  | NUMBER(4, 0) | YES | Number of S phase readings with non-zero output weights
nbfm |  | NUMBER(4, 0) | YES | Number of P first motions with non-zero input weights
locevid |  | VARCHAR2(12) | YES | Local event identifier. This attribute describes the original event identifier of the event. In combination with auth and subsource, it can be used to uniquely identify the original event identifier from that source. For example, waveforms from the original source may be associated with this identifier
quality |  | NUMBER(2, 1) | YES | This attribute denotes the quality of an origin, an arrival, or a mechanism. 1.0 = good, 0.0 = bad
fdepth |  | VARCHAR2(1) | YES | This attribute indicates if the depth was fixed or not to compute the solution
fepi |  | VARCHAR2(1) | YES | This attribute indicates if the epicenter was fixed or not to compute the solution
ftime |  | VARCHAR2(1) | YES | This attribute indicates if the origin time was fixed or not to compute the solution
vmodelid |  | VARCHAR2(2) | YES | Velocity model identification. This string identifies a version (instance) of the velocity model for the specified domain and algorithm. This version should be changed whenever the velocity model is changed. It is recommended that values 00 - 99 be used for this field
cmodelid |  | VARCHAR2(2) | YES | Velocity model domain. This string identifies the organization responsible for the velocity model. Recommendations for this field are the SEED network name, or a unique abbreviation of the processing center when using data from multiple networks
rflag |  | VARCHAR2(2) | YES | This flag describes whether an observation was generated automatically, by a human, or has been saved, finalized or canceled
crust_type |  | VARCHAR2(1) | YES | The type of crust model used for travel time calculations. Each type has its own geometry of velocity layers or gradients within layers, tied to the options of the location program
crust_model |  | VARCHAR2(3) | YES | The code for the regional (geographic) crust model that is dominant in the travel time calculations. The crust model depends on the location of the earthquake origin and not on the recording station. The code is for the highest weighted model if more than one is used
gtype |  | VARCHAR2(1) | YES | Geographic type (local, regional, teleseism)
lddate |  | DATE | YES | Load date. Date and time that the record was created, in Oracle date datatype

origin Primary and Unique Keys

Key Name | Key Type | Keys
orkey01 | PrimaryKey | orid

origin Foreign Keys

Parent Relationships:

Table Name | Type | Cardinality | Constraint Name | VerbPhrase | InversePhrase | Foreign Keys | Is Supertype | Deferrable | Initially Deferred
event | Non-Identifying | One To Zero or More | Ori_Eve |  |  | evid | NO | NO | NO
mec | Non-Identifying | Zero or One to Zero or More | Ori_Mec |  |  | prefmec | NO | NO | NO
netmag | Non-Identifying | Zero or One to Zero or More | Ori_Net |  |  | prefmag | NO | NO | NO

Child Relationships:

Table Name | Type | Cardinality | Constraint Name | VerbPhrase | InversePhrase | Foreign Keys | Is Subtype | Deferrable | Initially Deferred
eventprefor | Non-Identifying | One To Zero or More |  |  |  |  | NO | NO | YES
remark origin | Identifying | One To Zero or More |  |  |  |  | NO | NO | YES
assocaro | Identifying | One To Zero or More | Aao_Ori |  |  |  | NO | NO | NO
assoccoo | Identifying | One To Zero or More | Aco_Ori |  |  |  | NO | NO | NO
assocamo | Identifying | One To Zero or More | Amo_Ori |  |  |  | NO | NO | NO
event | Non-Identifying | One To Zero or More | Eve_Ori |  |  |  | NO | NO | NO
mec | Non-Identifying | One To Zero or More | Mec_Ori |  |  |  | NO | NO | NO
mec | Non-Identifying | One To Zero or More | Mec_Ori2 |  |  |  | NO | NO | NO
netmag | Non-Identifying | One To Zero or More | Net_Ori |  |  |  | NO | NO | NO
origin_error | Identifying | One To Zero or More | Ori__Err_Ori |  |  |  | NO | NO | NO

origin Check Constraints

Check Constraint Name | CheckConstraint
origin02 | datumhor in ('NAD27','WGS84')
origin03 | datumver in ('NAD27','WGS84','AVERAGE')
origin04 | depth >= -10.0 and depth <= 1000.0
origin05 | distance >= 0.0
origin06 | erhor >= 0.0
origin07 | erlat >= 0.0
origin08 | erlon >= 0.0
origin09 | fdepth in ('y','n')
origin10 | fepi in ('y','n')
origin11 | ftime in ('y','n')
origin12 | gap >= 0.0 and gap <= 360.0
origin15 | nbfm >= 0
origin16 | nbs >= 0
origin17 | ndef >= 0
origin18 | orid > 0
origin19 | quality >= 0.0 and quality <= 1.0
origin20 | type in ('H','h','C','c','A','a','D','d','u','U')
origin21 | stime >= 0.0
origin23 | wrms >= 0.0
origin24 | sdep >=0.0
origin25 | totalarr >=0
origin26 | totalamp >= 0
origin28 | rflag in ('a','h','f','A','H','F','i','I','c','C')
origin30 | crust_type in ('H','T','E','L','V')
origin31 | gtype in ('L','R','T')