30 June 2003 [~public/geodesy/stations/cencalif/douglas]

STATION DESCRIPTION

NETWORK:Benito COUNTY:FRESNO

STATION CODE: DGLS QUAD:LEVIS, CA

STAMPING:DOUGLAS 1962

TYPE:Disk SET BY:USCGS

CENTER MARK:

COORDINATES: 36.58900°N, 120.49414°W PID:GU0874

36°35’20.4" 120°29’38.9"

GENERAL LOCATION: Is in the NE corner of a farm implement yard, about 13 miles SW of Mendota and 14 miles WSW of Tranquility.

TO-REACH ROUTE DESCRIPTION: From the jct of State Hwy 180 and 33 in the N edge of Mendota, go S on State Hwy 33 for 8.75 miles to the intersection of Adams Avenue and a sign "TRANQUILITY" to the left. Turn right on Adams Avenue and go W for 6 miles to the intersection with Douglas Avenue. Turn left on Douglas Avenue and go S for 2.75 miles to a transmission line tower and the azimuth mark on the right. Continue southerly on Douglas Avenue for 0.25 mi to a crossroad and some farm buildings on the left. Turn left on Dinuba Avenue, dirt road for 0.05 mi to the station on the right.

STATION MARK DESCRIPTION: Station mark is a standard disk, stamped DOUGLAS 1962, set in the top of an 11 inch square concrete post projecting 2 inches. It is 300.8 feet east-southeast of a transformer pole, 153 feet southwest of a powerline pole, 89 feet south of the centerline of a dirt road and 2.4 feet south- southeast of a witness post.

Reference mark 1 is a standard disk, stamped DOUGLAS NO 1 1962, set in the top of an 11 inch square concrete post projecting 5 inches. It is 19.8 feet south of the centerline of the road and 1.9 feet west-southwest of the powerline pole. it is about 4 feet lower than the station.

Reference mark 2 is a standard disk, stamped DOUGLAS NO 2 1962, cemented in a drill hole in a 3 x 8 foot concrete foundation projecting 2 feet. It is 25 feet west-northwest of where a north-south and east-west row of trees meet. It is about 2 feet lower than the station.

ACCESS NOTES (KEYS etc):

MISCELLANEOUS INFORMATION: Mark not found in 1967−not used in 1982 survey. Not used in 1998 survey.

REFERENCE MARKS:

Name Distance (m) Azimuth (deg) DOUGLAS RM 1 51.520 58.45 DOUGLAS RM 2 54.560 145.07

Dockter 1998: did not visit. Looked like low priority.

- 1 -